Directions for Assembly of Passport to Concord Natural Lands PDF

For Double-Sided Printing:

1. Print entire passport double sided
2. Cut each 8.5 x 11 sheet across the middle into two 5.5 x 8.5 pieces
3. Fold each of those pieces in half down the middle
4. Put pages into order according to the numbers on the bottom
5. Staple on the crease

(If you cannot print double sided, print the odd pages first, then put the paper back in the printer so it will come out again and print the even pages)